|  |  |
| --- | --- |
| Product Title | [**KuDoS**](https://www.dranetz.com/product/dranetz-hdpq-guide-power-quality-analyzer/) **– Hydraulic Crimpers** |
| Product Tagline | *Professional Electric & Electronic Tool hand Tools* |
| Gambar Utama Produk |  |
| Product Brand | *A picture containing text, tableware, dishware, plate  Description automatically generated* |
| Overview Product | *Hydraulic Crimping Tools for Steel, Copper and Aluminium Lugs / Conductors*  |
| PDF Brosur | *https://www.dropbox.com/s/26q66z5g6fshcmu/KuDos\_Catalogue.pdf?dl=0* |
| Product Details | 1. Model No. HH-400

Length : 559 mmWeight : 5.8 kgs (Dies not included)■ Specifications :Max. Pressure : 700 barOil Required : 57 ccMax. Output : 15.82 tons / 140.7 kN ■ Features :Light weight, compact and slim design.Single stage pumping for rapid ram advance.Relief valve.Head rotates through 180° for difficult working environment. ■ Accessories :Plastic carrying case※Crimping tope only without any die set.※Dies sold separately1. Model No. 9H-150

Length : 528 mmWeight : 5.0 kgs■ Specifications :Max. Pressure : 700 barOil Required : 31 ccMax. Output : 14.01 tons / 124.6 kN ■ Crimping Capacity :For non-Insulated terminals and sleeves up to 150 mm²With Indentor 14, 22, 38~70 and 80~150 mm² ■ Features :Light weight, compact and slim design.Rotary nest for easy setting.Two stage pumping for rapid ram advance.Relief valve. ■ Accessories :Plastic carrying case1. Model No. HYCP-185

Length : 373 mmWeight : 2.1 kgs ■ Specifications :Max. Pressure : 550 barOil Required : 16 ccMax. Output : 5.85 tons / 52.0 kNCrimping CapacityAccepts BEKU type diesStock Dies are for DIN 46235 terminals※Dies sold separately (AHE-1016/2535/5070/95120/150/185) ■ Features :Light weight, compact and slim design.Single action cylinder with spring return.Accepts BEKU type dies.Yoke and Latch type head for easy die changes and removal of connectors.Adjustable ram stroke, 10-15 mm to minimize pumping action.Built-ln bypass relief valve.Small handle spread for close quarter applications. ■ Accessories :Plastic carrying case1. Model No. UC-6

Length : 627 mmWeight : 6.0 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 27 ccMax. Output : 7.03 tons / 62.5 kNJaw Opening : 29 mmMax. Crimping Capacity: up to 32 mm outer diameter connector (UC-6) ■ Features :Light weight, compact and slim design.Pressure relief valve for overload protection.Automatic low/high-pressure conversion with rapid/slow operating motion.360° rotating head for convenient operation.Two-stage hydraulic system reduces the number of pumps required.Dieless compression to crimp Anderson style connectors up to 500 MCM. ■ Accessories :Plastic carrying case1. Model No. UB-400

Height : 598 mmWeight : 6.8 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 48 ccMax. Output : 14.01 tons / 124.6 kNJaw Opening : 26 mm ■ Crimping Capacity :Max. Compression : 400mm² copper / aluminum lugs.Accepts all dies used for Alcoa, Burndy, T&B, Klauke, Cembreand Blackburn 6 tons compressors.※Dies sold separately(CU16/25/35/50/70/95/120/150/185/240/300/400) ■ Features :330° rotating head for convenient operation.Fiberglass handles are durable and light weight.External adjustable relief valve.Pressure relief valve for overload protection.Automatic low/high-pressure conversion with rapid/slow operating motion.Two-stage hydraulic system reduces the number of pumps required. ■ Accessories :Plastic carrying case1. Model No. UB-412T

Length : 630 mmWeight : 6.4 kgs ■ Specifications :Max. Pressure : 700 bar Oil Required : 53 ccMax. Output : 12.87 tons / 114.5 kNJaw opening : 32 mm ■ Crimping Capacity :Max. Compression : 400mm² copper lugsAccepts all dies used for Alcoa, Burndy, T&B, Klauke, Cembreand Blackburn 6 tons compressors.※Dies sold separately(CU16/25/35/50/70/95/120/150/185/240/300/400) ■ Features :180° rotating head for convenient operation.Fiberglass handles are durable and light weight.External adjustable relief valve.Pressure relief valve for overload protection.Automatic low/high-pressure conversion with rapid/slow operating motion.Two-stage hydraulic system reduces the number of pumps required. ■ Accessories :Plastic carrying case |
| Key Features | *Hydraulic Crimpers* |
| Galeri Produk | *TERLAMPIR* |