|  |  |
| --- | --- |
| Product Title | [**KuDoS**](https://www.dranetz.com/product/dranetz-hdpq-guide-power-quality-analyzer/) **– Hydraulic Crimping Heads** |
| Product Tagline | *Professional Electric & Electronic Tool hand Tools* |
| Gambar Utama Produk |  |
| Product Brand | *A picture containing text, tableware, dishware, plate  Description automatically generated* |
| Overview Product | *Hydraulic Crimping Equipment for Steel, Copper and Aluminium Lugs / Conductors*  |
| PDF Brosur | *https://www.dropbox.com/s/26q66z5g6fshcmu/KuDos\_Catalogue.pdf?dl=0* |
| Product Details | 1. Model No. 9H-150HE

Length : 246 mmWeight : 2.7 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 31 ccMax. Output : 14.01 tons / 124.6 kN ■ Crimping Capacity :For non-insulated terminals and sleeves up to 150 mm²With indentors 14, 22, 38~70 and 80~150 mm² ■ Features :Light weight, compact and slim design.Rotary nest for easy setting.Operated by are hydraulic pump with rated oil pressure of 700 bar (10,000 psi).■ Accessories :Plastic carrying case1. Model No. UCP-240HE

Length : 213 mmWeight : 2.4 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 24 ccMax. Output : 9.73 tons / 86.6 kN ■ Crimping Capacity :Accepts BEKU type diesHex. Crimping : 10-240 mm²Cu sleeves&lugs NFC 20.130:20 to 240 mm²Cu or Al bare or insulated sleeve : E54 to E230Cu or Al sleeves&lugs DIN 48083 : KZ6 to KZ25Pre-rounding : 35 to 240 mm※Dies sold separately ■ Features :Light weight, compact and slim design.Operated by are hydraulic pump with rated oil pressure of 700 bar (10,000 psi). ■ Accessories :Plastic carrying case1. Model No. UB-400HE

Length : 260 mmWeight : 4.2 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 47 ccMax. Output : 14.01 tons / 124.6 kNJaw Opening : 26 mm ■ Crimping Capacity :Max. compression: 400 mm² copper lugsAccepts all dies used for Alcoa, Burndy, T&B, Klauke, Combre and Blackburn 12-ton compressors※Dies sold separately(CU16/25/35/50/70/95/120/150/185/240/300/400) ■ Features :C-frame has open jaw for easy access to the fitting.Operated by are hydraulic pump with rated oil pressure of 700 bar (10,000 psi).Single action cylinder with spring return.Dies are easy to change.Crimping capacity identical to UB-400 tool. ■ Accessories :Plastic carrying case1. Model No. UB-412THE

Length : 261 mmWeight : 4.2 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 53 ccMax. Output : 14.01 tons / 124.6 kNJaw Opening : 32 mm ■ Crimping Capacity :Max. compression : 400 mm² copper lugsAccepts all dies used for Alcoa, Burndy, T&B, Klauke, Combre and Blackburn 12-ton compressors※Dies sold separately(CU16/25/35/50/70/95/120/150/185/240/300/400) ■ Features :C-frame has open jaw for easy access to the fitting.Operated by any hydraulic pump with rated oil pressure of 700 bar (10,000 psi ).Single action cylinder with spring return.Dies are easy to change.Crimping capacity identical to UB-412T tool. ■ Accessories :Plastic carrying case1. Model No. UC-6HE

Length : 278 mmWeight : 3.2 kgs■ Specifications :Max. Pressure : 700 barOil Required : 27 ccMax. Output : 7.03 tons / 62.5 kNMax. Crimping capacity : up to 32 mm outer diameter connector(UC-6)■ Features :Light weight, compact and slim design.Operated by any hydraulic pump with rated oil pressure of 700 bar(10,000 psi).Dieless compression to crimp Anderson style connectors up to 500 MCM.■ Accessories :Plastic carrying case1. Model No. HYCP-451000HE

Length : 258 mmWeight : 11.6 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 226 ccMax. Output : 49.25 tons / 438.1 kNRam Stroke : 35.5 mm ■ Crimping Capacity :Max. crimping capacity: 1000 mm²Customized die sets can be orderedCU 400/500/630/800/1000 sold separately ■ Features :U-type head design is solid and durableLock pin design holds die firmly in place.Operated by any hydraulic pump with rated oil pressure of 700 bar (10,000 psi).Single action cylinder with spring return. ■ Accessories :Plastic carrying case■ Model No . ADP-451000HEThis adapter is designed for hydrauliccompression head HYCP-451000HE / HYCP-451000D to interchange with 12-ton(up to 400 mm²)1. Model No. HYCP-60D

Length : 446 mmWeight : 23.3 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 298 ccMax. Output : 60.81 tons / 541.0 KnRam Stroke : 38 mm ■ Crimping Capacity :Crimping range : up 60 mm O.D.sleeveAccepts all dies used for Alcoa, 60 ton compressorsDouble-acting hydraulic pump required※Dies are manufactured on request only ■ Features :Solid metal loop at base for hoist work.Ram retracts hydraulically; the ram retracting time is 1/3 of spring return.Operated by any double-acting hydraulic pump with rated oil pressure of 700 bar (10,000 psi).Detachable ground stand as a standard accessory.Large handle for easy carrying.Compression head is designed as a portable tool for installing compression sleeves and terminals for transmission construction and/or maintenance work. ■ Accessories :Metal case1. Model No. SR-100C

Length : 364 mmWeight : 31.4 kgs ■ Specifications :Max. Pressure : 700 barOil Required : 318 ccMax. Output : 110.82 tons / 985.9 KnRam Stroke : 22 mm ■ Crimping Capacity :Crimping range :Copper : up to 64 mm O.D.sleeveAluminum : up to 71 mm O.D.sleeveSteel : up to 32 mm O.D.sleeve※Double-acting hydraulic pump required※Dies are manufactured on request only ■ Features :Operated by any hydraulic pump with rated oil pressure of 700 bar (10,000 psi).Functional handles for easy carrying and repositioning.Removable die cap for easy connector positioning.Ram retracts hydraulically ; the ram retracting time is 1/3 of spring return.Compression head is designed as a portable tool for installing compression sleeves and terminals for transmission construction and/or maintenance work.1. Model No. 200W

Length : 445 mmWeight : 78.0 kgs ■ Specifications :Max. Pressure : 700 barOil required : 1049 ccMax. output : 219.51 tons / 1952.9 kNRam stroke : 37 mm ■ Crimping Capacity :Crimping range :Copper : up to 86 mm O.D.sleeveAluminum : up to 100 mm O.D.sleeveSteel : up to 50 mm O.D.sleeve※Double-acting hydraulic pump required※Dies are manufactured on request only or current die set available sold separately ■ Features :Operated by any hydraulic pump with rated oil pressure of 700 bar (10,000 psi).Functional handles for easy carrying and repositioning.Removable die cap for easy connector positioning.Ram retracts hydraulically ; the ram retracting time is 1/3 of spring return.Compression head is designed as a portable tool for installing compression sleeves and terminals for transmission construction and/or maintenance work.1. Model No. SR-300CX

Length : 682 mmWeight : 182.0 kgs■ Specifications :Max. Pressure : 700 barOil Required : 3340 ccMax. Output : 350.24 tons / 3115.9 kNRam Stroke : 43.7 mm■ Crimping Capacity :Maximum compressible sleeve diameter : 150mm※Double-Acting hydraulic pump required.※Dies are manufactured on request only.■ Features :Operated by any double-acting hydraulic pump with rated oil pressure of 700 bar (10,000 psi).Functional handles for easy carrying and repositioning.Removable die cap for easy connector positioning.Ram retracts hydraulically; the ram retracting time is 1/3 of spring return.Compression head is designed as a portable tool for installing compression sleeves and terminals for transmission construction and / or maintenance work.※ Crimping without die sets is prohibited. |
| Key Features | *Hydraulic Crimping Heads* |
| Galeri Produk | *TERLAMPIR* |