|  |  |
| --- | --- |
| Product Title | [**KuDoS**](https://www.dranetz.com/product/dranetz-hdpq-guide-power-quality-analyzer/) **– Hydraulic Pumps** |
| Product Tagline | *Professional Electric & Electronic Tool hand Tools* |
| Gambar Utama Produk |  |
| Product Brand | *A picture containing text, tableware, dishware, plate  Description automatically generated* |
| Overview Product | *Hydraulic Pumps for Crimping Head, Cutting Head, Punching Head, Bender head and Splitting Head* |
| PDF Brosur | *https://www.dropbox.com/s/26q66z5g6fshcmu/KuDos\_Catalogue.pdf?dl=0* |
| Product Details | 1. Model No. HP-700A

Hand Pump SeriesLength : 595 mmWeight : 8.8 kgs ■ Specifications :Max. pressure : 700 barOil required : 720 cc■ Oil delivery :12.26 cc / stroke at low pressure2.26 cc / stroke at high pressure ■ Features :Dual speed pump piston for rapid advance.Two stage pumping action.External adjustable pressure setting up to 700 bar.Internal oil bladder type oil reservoir allows operation in any position.Replaceable dropout bypass valve cartridge tor easy rapier.Economical yet dependable hydraulic foot pump. ■ Accessories :2M hydraulic hose attached1. Model No. HYP-700FT

Foot Pump SeriesLength : 720 mmWeight : 13.5 kgs ■ Specifications :Max. pressure : 700 barOil required : 1000 cc■ Oil delivery :35.8 cc / stroke at low pressure2.1 cc / stroke at high pressure ■ Features :Dual speed pump piston for rapid advance.Two stage pumping action.External adjustable pressure setting up to 700 bar.Internal oil bladder type oil reservoir allows operation in any position.Replaceable dropout bypass valve cartridge tor easy repair.Economical yet dependable foot hydraulic pump. ■ Accessories :2M hydraulic hose attached1. Model No. CEP-15SS

Electrical Pump SeriesHeight : 319 mmWeight : 8.0 kgs (w/o battery) ■ Specifications :Max. pressure : 700 barOil required : 1500 cc■ Oil delivery :1.2 L / min at low pressure0.3 L / min at high pressure ■ Features :Pressure and operation data of date by display function.Programming switch for crimping, cutting or lifting propose on the panel.Warning Function: Buzzer alert at long deep if crimping not complete and losing pressure when failure caused.Display related pumping pressure and battery capacity.Environmentally design for saving energy as automatic switch to sleep mode after 3 mins without any activate action.Interior counting function attachedPSI / BAR unit available.Shoulder strap for high wearing comfort ■ Accessories :18V battery 4.0Ah110V or 230V charger1M hydraulic hose attached1. Model No. EP-30MD

Electrical Pump SeriesHeight : 454 mmWeight : 14.1 kgs (w/o oil) ■ Specifications :Max. pressure : 700 barOil required : 3000 cc4 way, 3 position manual valveDrive unit : 220V/AC or 110V/AC 50/60Hz ■ Oil delivery :2.6 L / min at low pressure0.32 L / min at high pressure ■ Features :With 5 meter remote control cable provides the user complete control to advance and retract.Two speed high performance.Pressure holds at 700 bar, ideal for maintenance and construction.Equipped with large-capacity one piece metal oil tank. ■ Accessories :Hydraulic hose should be ordered separately.1. Model No. EP-76SS

Electrical Pump SeriesHeight : 480 mmWeight : 26.6 kgs (w/o oil) ■ Specifications :Max. pressure : 700 barOil required : 8000 cc3 way, 2 position manual valveDrive unit : 220V/AC 100V~120V, 210V~240V, 50/60Hz, 1/2Hp ■ Oil delivery :3.9L / min at low pressure0.2L / min at high pressure ■ Features :With 5 meter remote control cable provides the user complete control to advance and retract.Two speed high performance.Equipped with single-phase, thermal protected induction motor to reduce noise level.Pressure holds at 700 bar, ideal for maintenance and construction.Equipped with large-capacity one piece metal oil tank. ■ Accessories :Hydraulic hose should be ordered separately.1. Model No. GHP-5

Engine Pump SeriesHeight : 590 mmWeight : 50.5 kgs (w/o oil) ■ Specifications :Max. pressure : 700 barOil required : 9.5LMotor size : 6.5HPValve type : 4 way, 3 positionMotor manufacturer : HondaManually controlled engine ■ Oil delivery :13.4L / min at low pressure2.4L / min at high pressure ■ Features :Pressure gauge can be located in upright position for better reading.Equipped with a 4 way, 3 position manual valve to prevent the electric control valve being locked and not able to perform retire because of high temperature.Supplied with a rack with rollers.High efficiency and fast working gasoline pump.1. Model No. EP-200SD

Engine Pump SeriesHeight : 691 mmWeight :78.4 kgs (w/o oil) ■ Specifications :Max. pressure : 700 barOil required : 20LMotor size : 2HPValve type : 4 way, 3 position solenoid valveInput:220V / 230V ■ Oil delivery :10.5L / min at low pressure1.0L / min at high pressure ■ Features :With 5 meter remote control cable provides the user complete control to advance and retract.Easy to use by one button control to advance and retract pumping.Two stage pumping of high performance.Equipped with single-phase, thermal protected motor to reduce noise level.Equipped with large-capacity one piece metal oil tank.  |
| Key Features | *Hydraulic Pumps* |
| Galeri Produk | *TERLAMPIR* |