|  |  |
| --- | --- |
| Product Title | [**KuDoS**](https://www.dranetz.com/product/dranetz-hdpq-guide-power-quality-analyzer/) **– Hydraulic Nut Splitters** |
| Product Tagline | *Professional Electric & Electronic Tool hand Tools* |
| Gambar Utama Produk |  |
| Product Brand | *A picture containing text, tableware, dishware, plate  Description automatically generated* |
| Overview Product | *Hydraulic Nut Spliter suitable for hexagonal grade 8 nuts* |
| PDF Brosur | *https://www.dropbox.com/s/26q66z5g6fshcmu/KuDos\_Catalogue.pdf?dl=0* |
| Product Details | 1. Model No. PF-1319   Length : 333 mm  Weight : 2.1 kgs  ■ Specifications :  Max. Pressure : 600 bar  Oil Required : 17 cc  Max. Output : 7.45 ton / 66.3 Kn  Bolting Range : M6~M12  (Hex. Nut range : 10-19 mm)  ■ Bolting Capacity :  Jaw opening : 24.3 mm  Ram Stroke : 17.3 mm  ■ Features :  Light weight, compact and slim design.  180° degree rotating head for convenient operation.  Single stage pumping.  Relief valve.  ■ Accessories :  Carrying Bag  ※Caution :  Only suitable for ≤ grade 8 nuts, splitting of stainless, square, and / or star nuts are prohibited.  Nut hardness must not exceed HRc-44.   1. Model No. HYNC-4510   HYNC-series (Single blade)    ■ Features :  Compact design.  Easy to use.  Seven models of nut splitter to choose from.  Unique angled head design for a variety of applications.  Single action cylinder with hydraulic advance with spring-return.  Operated by hydraulic pump with rated oil pressure of 700 bar(10,000psi).  Specifications : Single blade type   |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | Model No | Bolt Range | Hex Nut Range (mm) | Capacity (ton) | Oil Capacity(cm³) | Dimensions(mm) | | | Net Weight(kg) | Gross Weight(kg) | | Length | Width | Height | | HYNC-1319 | M6-M12 | 10-19 | 6.23 | 15 | 170 | 40 | 48 | 1.2 | 2.6 | | HYNC-1924 | M12-M16 | 19-24 | 11.24 | 20 | 191 | 54 | 62 | 2.0 | 3.6 | | HYNC-2432 | M16-M22 | 24-32 | 18.39 | 60 | 222 | 64 | 72 | 3.0 | 5.2 | | HYNC-3241 | M22-M27 | 32-41 | 25.69 | 80 | 244 | 75 | 88 | 4.4 | 7.0 | | HYNC-4150 | M27-M33 | 41-50 | 38.92 | 155 | 288 | 94 | 105 | 8.2 | 13.6 | | HYNC-5060 | M33-M39 | 50-60 | 54.88 | 240 | 318 | 106 | 128 | 11.8 | 18.4 | | HYNC-6075 | M39-M48 | 60-75 | 102.76 | 492 | 393 | 156 | 181 | 34.1 | 42.7 |      |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | Model No | A | B | C | D | E | F | G |  | Spare Chisels No. | | | HYNC-1319 | 40 | 21 | 7 | 19 | 50 | 29 | 120 | HYNC-1319#4 | Chisels | | HYNC-1924 | 54 | 25 | 10 | 25 | 62 | 40 | 146 | HYNC-1924#4 | Chisels | | HYNC-2432 | 64 | 33 | 13 | 30 | 76 | 52 | 180 | HYNC-2432#4 | Chisels | | HYNC-3241 | 70 | 42 | 16 | 36 | 87 | 65 | 205 | HYNC-3241#4 | Chisels | | HYNC-4150 | 90 | 52 | 21 | 45 | 108 | 76 | 245 | HYNC-4150#4 | Chisels | | HYNC-5060 | 106 | 60 | 24 | 54 | 125 | 92 | 288 | HYNC-5060#4 | Chisels | | HYNC-6075 | 156 | 80 | 27 | 75 | 184 | 110 | 365 | HYNC-6075#4 | Chisels |   ※Caution : Only suitable for ≤ grade 8 nuts, splitting of stainless, square, and / or star nuts are prohibited. Nut hardness must not exceed HRc-44.  ■ Accessories :   |  |  |  | | --- | --- | --- | | Model No. | Hex Wench(mm) | Packaging | | HYNC-1319 | 2.5 & 4 | KuDos ® Plastic Carrying Case | | HYNC-1924 | 3 & 5 | | HYNC-2432 | 3 & 5 | | HYNC-3241 | 4 & 6 | | HYNC-4150 | 4 & 6 | | HYNC-5060 | 5 & 6 | | HYNC-6075 | 5 & 6 | Crate |  1. Model No. HYNC-4150D   HYNC-series (Double blade)    ■ Features :  Compact design.  Easy to use.  Seven models of nut splitter to choose from.  Unique angled head design for a variety of applications.  Single action cylinder with hydraulic advance with spring-return.  Operated by hydraulic pump with rated oil pressure of 700 bar(10,000psi).  Specifications : Double blade   |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | Model No | Bolt Range | Hex Nut Range (mm) | Capacity (ton) | Oil Capacity(cm³) | Dimensions(mm) | | | Net Weight(kg) | Gross Weight(kg) | | Length | Width | Height | | HYNC-1319D | M6-M12 | 10-19 | 6.23 | 15 | 223 | 44 | 67 | 1.3 | 2.8 | | HYNC-1924D | M12-M16 | 19-24 | 11.77 | 20 | 250 | 56 | 74 | 2.4 | 3.8 | | HYNC-2432D | M16-M22 | 24-32 | 19.07 | 60 | 275 | 64 | 78 | 3.5 | 5.4 | | HYNC-3241D | M22-M27 | 32-41 | 26.49 | 80 | 305 | 77 | 90 | 5.1 | 7.2 | | HYNC-4150D | M27-M33 | 41-50 | 38.92 | 155 | 344 | 97 | 111 | 9.7 | 13.8 | | HYNC-5060D | M33-M39 | 50-60 | 56.04 | 240 | 386 | 115 | 131 | 14.7 | 18.6 | | HYNC-6075D | M39-M48 | 60-75 | 102.76 | 492 | 476 | 170 | 186 | 40.7 | 42.9 |      |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | Model No | A | B | C | D | E | F | G |  | Spare Chisels No. | | | HYNC-1319D | 40 | 21 | 18 | 19 | 53 | 41 | 139 | HYNC-1319D#7、#10 | Chisels | | HYNC-1924D | 54 | 26 | 22 | 25 | 66 | 50 | 168 | HYNC-1924D#7、#10 | Chisels | | HYNC-2432D | 64 | 34 | 26 | 30 | 78 | 65 | 198 | HYNC-2432D#7、#10 | Chisels | | HYNC-3241D | 77 | 43 | 31 | 36 | 90 | 80 | 231 | HYNC-3241D#7、#10 | Chisels | | HYNC-4150D | 94 | 52 | 39 | 45 | 111 | 93 | 271 | HYNC-4150D#7、#10 | Chisels | | HYNC-5060D | 106 | 62 | 43 | 54 | 131 | 107 | 315 | HYNC-5060D#7、#10 | Chisels | | HYNC-6075D | 156 | 77 | 54 | 75 | 186 | 133 | 411 | HYNC-6075D#7、#10 | Chisels |   ※Caution : Only suitable for ≤ grade 8 nuts, splitting of stainless, square, and / or star nuts are prohibited. Nut hardness must not exceed HRc-44.  ■ Accessories :   |  |  |  | | --- | --- | --- | | Model No. | Hex Wench(mm) | Packaging | | HYNC-1319D | 2.5 & 4 | KuDos ® Plastic Carrying Case | | HYNC-1924D | 3 & 5 | | HYNC-2432D | 4 & 6 | | HYNC-3241D | 4 & 6 | | HYNC-4150D | 4 & 6 | | HYNC-5060D | 5 & 6 | | HYNC-6075D | 5 & 6 | Crate | |
| Key Features | *Hydraulic Nut Splitter* |
| Galeri Produk | *TERLAMPIR* |